rtsp://user name:password@ip address:rtsp prot/0  main stream
rtsp://user name:password@ip address:rtsp prot/1  sub stream
rtsp://user name:password@ip address:rtsp prot/2  third stream